**LR 21-D** (1968) **FODEN CONCRETE TRUCK**

|  |  |  |
| --- | --- | --- |
| © year on base: nonescale: 1:89 (not cast on base)length: 76mmwidth: 28mmheight: 38mmMATCHBOX lettering on base: noneadditional lettering on base: nonecompany on base: MADE IN ENGLAND BY LESNEYnumber on base: 21cast license plate: none | no interiorplastic barrel & cogplastic wheelsdome head rounded axlesRola-matic action (barrel) |  |

| **#** | **cab** | **chassis** | **barrel / cog** | **windows** | **wheels** | **deco** | **chassis type** | **base hole** | **mixer pin** | **axle braces** | **sub-var** | **note** | **cate** | **area** | **Stannard #** | **Jones #** | **date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0010 | med. yellow | red metal E | yellow | green | 11.5x45 black | none | chassis 1 | **no** | metal axle pin | **none** | x | #21 |  |  | 01 | 01 | 1968 |
| 0020 | med. yellow | red metal E | yellow | green | 11.5x45 black | none | chassis 1 | **no** | metal axle pin | **narrow** | x | #21 |  |  | 02 | 02 | 1968 |
| 0030 | med. yellow | red metal E | yellow | green | 11.5x45 black | none | chassis 1 | yes | plastic | wide |  | #21 |  |  |  | 03 | 1969 |
| 0040 | med. yellow | red metal E | yellow | green | 11.5x45 black | none | chassis **2** | yes | plastic | wide |  | #21 |  |  |  | 04 | 1969 |
| 0050 | med. yellow | red metal E | yellow | green | 11.5x45 black | none | chassis 3 | yes | plastic | wide | x | #21 |  |  | 03 | 05 | 1969 |
| 0060 | med. yellow | **dull** red metal E | yellow | green | 11.5x45 black | none | chassis 3 | yes | plastic | wide | x | #21 |  |  |  |  | 1969 |
| 0065 | **lt.** yellow | red metal E | yellow | green | 11.5x45 black | none | chassis 3 | yes | plastic | wide | x | #21 |  |  |  |  | 1969 |
| 0070 | med. yellow | red metal E | yellow | green | 11.5x45 black | none | chassis **4** | yes | **countersunk** plastic | wide | x | #21 |  |  | 04 | 06 | 1971 |
| 0080 | **lemon** | red metal E | yellow | green | 11.5x45 black | none | chassis **4** | yes | **countersunk** plastic | wide |  | #21 |  |  |  |  | 1971 |

| **chassis type code** | **ladder at rear left side** | **rear platforms** | **braces below rear platforms** |
| --- | --- | --- | --- |
| chassis 1 | straight | thin | no |
| chassis 2 | straight | **thick** | no |
| chassis 3 | **tapered** on top right side | thin | no |
| chassis 4 | **tapered** on top right side | thin | **yes** |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **21D** |  |  |  |

**Previous ref.: none**

**Later ref.: ⇒ ⇒ ⇒ LS 21-A FODEN CONCRETE TRUCK**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | E4 | light blue sides, color picture with "MATCHBOX" on end flaps, with NEW MODEL, ®, flags on inner end flaps |  |  | 1968 |
| 02 | F | without NEW, A LESNEY PRODUCT, trademark on end flaps, no MARK on end flaps |  |  | 1969 |
| 03 | F | without NEW, LESNEY PRODUCTS & CO. LTD. ..., trademark on end flaps, no MARK on end flaps |  |  | 1970 |
| 04 | F | without NEW, "MATCHBOX" REG'D T.M. ..., no trademark on end flaps, no MARK on end flaps |  |  | 1970 |