**LR 58-B** (1962) **International DROTT EXCAVATOR**

|  |  |  |
| --- | --- | --- |
| © year on base: nonescale: 1:60 (not cast on base)length: 65mmwidth: 32mmheight: 25mmMATCHBOX lettering on base: noneadditional lettering on base: nonecompany on base: MADE IN ENGLAND BY LESNEYnumber on base: 58cast license plate: none | metal base & enginemetal shovel swivelsno interiorno windowsdome head rounded axlesrubber tracks |  |

| **#** | **body** | **shovel** | **base / engine** | **rollers** | **tracks** | **deco** | **shovel arms** | **arm thickness** | **arm stops** | **base wedges** | **sub-var** | **note** | **cate** | **area** | **Stannard #** | **Jones #** | **date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0010 | red | red | silver-gray E | 9.5mm unpainted **metal** | 25 tread green | none | **open** | 1mm **thin** | no | **no** |  | #58 |  |  |  | 01 | 1962 |
| 0020 | red | red | silver-gray E | 9.5mm black plastic | 25 tread green | none | **open** | 1mm **thin** | no | **no** | x | #58 |  |  | 01 | 02 | 1962 |
| 0030 | red | red | silver-gray E | 9.5mm black plastic | 25 tread green | none | **open** | 1.3mm thick | no | **no** | (x) | #58 |  |  | 02 | 03 | 1963 |
| 0040 | red | red | silver-gray E | 9.5mm black plastic | 25 tread green | none | **open** | 1.3mm thick | no | yes | x | #58 |  |  | 03 | 04 | 1963 |
| 0050 | **dk.** red | **dk.** red | silver-gray E | 9.5mm black plastic | 25 tread green | none | **open** | 1.3mm thick | no | yes | (x) | #58 |  |  |  |  | 1963 |
| 0060 | red | red | silver-gray E | 9.5mm black plastic | 25 tread green | none | closed | 1.3mm thick | no | yes | x | #58 |  |  | 04 | 05 | 1964 |
| 0070 | red | red | silver-gray E | 9.5mm **silver** plastic | 25 tread green | none | **open** | 1.3mm thick | no | yes | (x) | #58 |  |  | 05 | 06 | 1963 |
| 0080 | red | red | silver-gray E | 9.5mm **silver** plastic | 25 tread green | none | closed | 1.3mm thick | no | yes | x | #58 |  |  | 06 | 07 | 1964 |
| 0090 | **orange** | **orange** | silver-gray E | 9.5mm black plastic | 25 tread green | none | closed | 1.3mm thick | **yes** | yes | x | #58 |  |  | 07 | 08 | 1965 |
| 0100 | **orange** | **orange** | **orange** E | 9.5mm black plastic | 25 tread green | none | closed | 1.3mm thick | **yes** | yes | x | #58 |  |  | 08 | 09 | 1966 |
| 0110 | **orange** | **orange** | **orange** E | 9.5mm **silver** plastic | 25 tread green | none | closed | 1.3mm thick | **yes** | yes |  | #58 |  |  |  | 10 | 1966 |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **58B** |  |  |  |

**Previous ref.: none**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | D1 | one blue & one black side, end flap lettering with serifs, with NEW MODEL, ***inner end flaps unknown*** | small number 58 without serifs |  | 1962 |
| 02 | D1 | one blue & one black side, end flap lettering with serifs, without NEW MODEL, plain inner end flaps | very small number 58 with serifs |  | 1962 |
| 03 | D2 | one blue & one black side, end flap lettering without serifs, without NEW MODEL, ***inner end flaps unknown*** | large number 58 with serifs |  | 1963/64 |
| 04 | D2 | two blue sides, end flap lettering without serifs, without NEW MODEL, flags on inner end flaps | large number 58 with serifs |  | 1965 |
| 05 | D2 | light blue sides, end flap lettering without serifs, without NEW MODEL, flags on inner end flaps | large number 58 with serifs |  | 1966 |
| 06 | E3 | light blue sides, color picture without "MATCHBOX" on end flaps, without NEW MODEL, no ®, flags on inner end flaps |  |  | 1966 |
| 07 | E4 | light blue sides, color picture with "MATCHBOX" on end flaps, without NEW MODEL, no ®, flags on inner end flaps |  |  | 1967 |