**LS 44-A** (1970) **G.M.C. REFRIGERATOR TRUCK**

|  |  |  |
| --- | --- | --- |
| © year on base: none  scale: 1:94 (not cast on base)  length: 76mm  width: 29mm  height: 37mm  MATCHBOX lettering on base: straight  additional lettering on base: SUPERFAST (straight)  company on base: LESNEY  number on base: 44  cast license plate: none | metal container  metal chassis is part of body  (A) at rear of base  PAT APP at rear of base  tow guide  no interior  black plastic wheels with silver hubs  gray plastic rear door opens  with rear door stop and rear bumper  short single removable plastic axle covers |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **#** | **body / chassis** | **container** | **grille / cab base** | **windows** | **wheels** | **deco** | **axle covers** | **sub-var** | **note** | **cate** | **area** | **Mack #** | **Mack date** | **date** |
| 01 | **red** E | **turquoise** | gray plastic | green | 4 spoke 11.5x2mm | none | black | f | #44 |  |  | 01 |  | 1970 |
| 06 | yellow E | **turquoise** | gray plastic | green | 4 spoke 11.5x2mm | none | black |  | #44 |  |  | 06 | 1993-03 | 1970 |
| 02 | yellow E | red | gray plastic | green | 4 spoke 11.5x2mm | none | black | f, r | #44 |  |  | 02 |  | 1970 |
| 04 | yellow E | red | gray plastic | green | 4 spoke 11.5x2mm | none | **red** | f, r | #44 |  |  | 04 |  | 1970 |
| f01 | yellow E | red | gray plastic | green | 4 spoke 11.5x2mm front, 4 spoke 11.5x**4**mm rear | none | black |  | #44 |  |  |  |  | 1971 |
| 03 | yellow E | red | gray plastic | green | 4 spoke 11.5x**4**mm | none | black | f | #44 |  |  | 03 |  | 1971 |
| 05 | yellow E | red | gray plastic | green | 4 spoke 11.5x**4**mm | none | **red** |  | #44 |  |  | 05 |  | 1971 |

**USA codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **MB 44-A** |  |  |  |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **44C** |  |  |  |

|  |  |
| --- | --- |
| **ROW numbers:** | **44** (1970-1971) |
| **USA numbers:** | **44** (1970-1971) |
| **Other numbers:** | **none** |

**NOTES:**

**Rear doors come with varying die numbers from 1 to 10.**

**Gray rear doors are prone to fading to gray-brown.**

**SUB-VARIATIONS:**

| **code** | **panel at container front** |
| --- | --- |
| f | flat |
| r | raised |

**Previous ref.: ⇒ ⇒ ⇒ LR 44-C G.M.C. REFRIGERATOR TRUCK**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | G | with NEW, red TM, "MATCHBOX" REG'D T.M. ..., SF parallel on sides, MARK 3 on end flaps, no SPECIFICATION... on end flaps |  |  | 1970 |
| 02 | G | with NEW, black TM, "MATCHBOX" REG'D T.M. ..., SF angled on sides, MARK 4 on end flaps, no SPECIFICATION... on end flaps |  |  | 1971 |
| 03 | G | with NEW, no TM, "MATCHBOX" REG'D T.M. ..., SF angled on sides, MARK 4 on end flaps, no SPECIFICATION... on end flaps |  |  | 1971 |