**LS 51-A** (1970) **(AEC) 8 WHEEL TIPPER**

|  |  |  |
| --- | --- | --- |
| © year on base: 1969scale: 1:92 (not cast on base)length: 76mmwidth: 27mmheight: 35mmMATCHBOX lettering on base: straightadditional lettering on base: SUPERFAST (straight), ERGOMATIC CABcompany on base: LESNEY. PROD & CO LTDnumber on base: 51cast license plate: none | plastic baselong single black removable plastic front axle coverPAT APP between front axle coverspat. no. 1052960 at front of dump basetow guideno interiorblack plastic wheels with silver hubsmetal dump tiltsmetal tailgate opens |  |

| **#** | **body / chassis** | **dump / tailgate** | **base** | **windows** | **wheels** | **deco** | **PAT APP** | **sub-var** | **note** | **cate** | **area** | **Mack #** | **Mack date** | **date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| f01 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | orange & white **DOUGLAS** labels | large |  | #51 |  |  |  |  | 1970 |
| f02 | lemon | silver-gray | **gray** E | blue | 5 slot 10x2mm | orange & white **DOUGLAS** labels | large |  | #51 |  |  |  |  | 1971 |
| 01 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | dk. green & yellow POINTER labels | large | **aashhh**, **aahsss**, (abhhhh),**bashhh**, **bahsss**, (**bahhss**),bahhhh, (bbssss), bbhhhh | #51 |  |  | 01 |  | 1970 |
| f09 | **lt. yellow** | silver-gray | silver E | blue | 5 slot 10x2mm | dk. green & yellow POINTER labels | large | abhhhh | #51 |  |  |  |  | 1970 |
| f07 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | dk. green & yellow POINTER labels left,**lt.** green & yellow POINTER labels right | large |  | #51 |  |  |  |  | 1970 |
| f08 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | **lt.** green & yellow POINTER labels left,dk. green & yellow POINTER labels right | large | abhhhh | #51 |  |  |  |  | 1970 |
| 02 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | **lt.** green & yellow POINTER labels | large | aahhhh, abhhhh, (bahhhh),**bbhhhs**, bbhhhh | #51 |  |  | 02 |  | 1970 |
| f04 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | **lt.** green & yellow POINTER labels | **small** | bbhhhh | #51 |  |  |  |  | 1971 |
| 04 | lemon | silver-gray | **gray** E | blue | 5 slot 10x2mm | dk. green & yellow POINTER labels | large |  | #51 |  |  | 04 |  | 1971 |
| 05 | lemon | silver-gray | **gray** E | blue | 5 slot 10x2mm | **lt.** green & yellow POINTER labels | large |  | #51 |  |  | 05 |  | 1971 |
| f06 | lemon | silver-gray | **gray** E | blue | 5 slot 10x2mm | **lt.** green & yellow POINTER labels | **small** |  | #51 |  |  |  |  | 1971 |
| 03 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | **none** | large | bahhhh | #51 |  |  | 03 |  | 1970 |
| f03 | lemon | silver-gray | silver E | blue | 5 slot 10x2mm | **none** | **small** | bbhhhh | #51 |  |  |  |  | 1971 |
| 06 | lemon | silver-gray | **gray** E | blue | 5 slot 10x2mm | **none** | large |  | #51 |  |  | 06 |  | 1971 |
| f05 | lemon | silver-gray | **gray** E | blue | 5 slot 10x2mm | **none** | **small** |  | #51 |  |  |  |  | 1971 |

**USA codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **MB 51-A** |  |  |  |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **51C** |  |  |  |

|  |  |
| --- | --- |
| **ROW numbers:** | **51** (1970-1971) |
| **USA numbers:** | **51** (1970-1971) |
| **Other numbers:** | **none** |

**NOTES:**

**Tailgates come with varying die numbers from 1 to 12 (top right corner).**

**Tailgates can be fitted in either of two ways (model number and die number inside or outside).**

**Same base as LS 10-A and LS 32-A.**

**SUB-VARIATIONS:**

| **Casting:** |  | **Wheels:** |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **code** | **dump base** | **chassis sides** |  | **code** | **first axle wheels** | **second axle wheels** | **third axle wheels** | **fourth axle wheels** |
| aa | block over dump guide wider on the left side | symmetric inside gaps in chassis sides |              | ssss | solid | solid | solid | solid |
| ab | block over dump guide wider on the left side | asymmetric inside gaps in chassis sides |  | sssh | solid | solid | solid | hollow |
| ba | block over dump guide wider on the right side | symmetric inside gaps in chassis sides |  | sshs | solid | solid | hollow | solid |
| bb | block over dump guide wider on the right side | asymmetric inside gaps in chassis sides |  | sshh | solid | solid | hollow | hollow |
|  |  |  |  | shss | solid | hollow | solid | solid |
|  |  |  |  | shsh | solid | hollow | solid | hollow |
|  |  |  |  | shhs | solid | hollow | hollow | solid |
|  |  |  |  | shhh | solid | hollow | hollow | hollow |
|  |  |  |  | hsss | hollow | solid | solid | solid |
|  |  |  |  | hssh | hollow | solid | solid | hollow |
|  |  |  |  | hshs | hollow | solid | hollow | solid |
|  |  |  |  | hshh | hollow | solid | hollow | hollow |
|  |  |  |  | hhss | hollow | hollow | solid | solid |
|  |  |  |  | hhsh | hollow | hollow | solid | hollow |
|  |  |  |  | hhhs | hollow | hollow | hollow | solid |
|  |  |  |  | hhhh | hollow | hollow | hollow | hollow |

**Previous ref.: ⇒ ⇒ ⇒ LR 51-C (AEC) 8 WHEEL TIPPER**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | G | with NEW, black TM, "MATCHBOX" REG'D T.M. ..., SF angled on sides, MARK 4 on end flaps, no SPECIFICATION... on end flaps |  |  | 1970 |
| 02 | G | with NEW, no TM, "MATCHBOX" REG'D T.M. ..., SF angled on sides, MARK 4 on end flaps, no SPECIFICATION... on end flaps |  |  | 1971 |