**MI 740** (1985) **HAY TRAILER**

other number: **MI 840**

|  |  |  |
| --- | --- | --- |
| © year on base: nonescale: 1:56 (not cast on base)length: 86mmwidth: 33mmheight: 37mmMATCHBOX lettering on base: straightadditional lettering on base: nonecompany on base: **none**number on base: nonecast license plate: none | metal base is part of bodyhigh letter A at rear of baseflat ejector ringsno interiorno windowsplastic wheelstwo plastic stakesmetal tow hitch turns |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **#** | **body / base** | **wheels** | **axles** | **deco** | **stakeclips** | **body casting** | **base casting** | **stakes** | **stake casting** | **sub-var** | **note** | **cate** | **area** | **Mack #** | **Mack date** | **date** |
| 0010 | red M | solid black 13x40 | press-fit | none | with | open holes in sides | no #, circles over axles | black | side clips, with top brace | x | TP-108 | TP |  |  |  | 1985 |
| 0020 | lt. yellow no origin | solid black 13x40 | press-fit | none | with | open holes in sides | no #, circles over axles | black | side clips, with top brace | x | TP-108MC-7 | TPMC |  |  |  | 19871988 |
| 0025 | **med.** yellow no origin | solid black 13x40 | press-fit | none | with | open holes in sides | no #, circles over axles | black | side clips, with top brace | x | MC-7 | MC |  |  |  | 1990 |
| 0030 | **dk.** yellow no origin | solid black 13x40 | press-fit | none | with | open holes in sides | no #, circles over axles | black | side clips, with top brace | x | MC-7 | MC |  |  |  | 1990 |

**USA codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **MB TP-108** |  |  |  |

|  |  |
| --- | --- |
| **ROW numbers:** | **none** |
| **USA numbers:** | **none** |
| **Other numbers:** | **none** |

**NOTE:**

**This model was not issued as a single in the basic range.**

**Previous ref.: ⇒ ⇒ ⇒ LR 40-C HAY TRAILER**

**Later ref.: none**